**BMC Firmware Update**

**Do not close the web gui during the update process.**

**1. Update through BMC web GUI**

1.1. default IP: 192.168.11.11 .

default account: admin

password: admin

1.2. Login to the BMC web gui,

1.3. Click the "Firmware Update" page.

1.4. Upload the firmware image file(\*.ima).

**2. Update through Yafuflash**

2.1. default IP: 192.168.11.11 .

default account: admin

password: admin

2.2. Full upgrade without Config Module preserved

$ Yafuflash -nw -ip <BMC IP Address> -u <Username> -p <Password> -force-boot <Firmware Filename>

2.3 Upgrade with Config Module preserved

$ Yafuflash -nw -ip <BMC IP Address> -u <Username> -p <Password> -preserve-config <Firmware Filename>