IPMITOOL.exe command options:

C:\Windows\Temp\Work2016\Utilities\ipmitool>cmd

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser sel list

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser sel elist

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser -v sel elist

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser sdr list

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser sdr elist

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser -v sdr elist

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser fru

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM IPMITOOL -I lan -H 192.168.22.22
 -U root -P superuser raw 0xXX 0xXX

C:\Windows\Temp\Work2016\Utilities\ipmitool>REM ipmitool -I ms (command)

C:\Windows\Temp\Work2016\Utilities\ipmitool>ipmitool -I ms  sdr elist
Could not enumerate class object (80041010)
Get Device ID command failed
Unable to open SDR for reading

C:\Windows\Temp\Work2016\Utilities\ipmitool>ipmitool
Commands:
        raw           Send a RAW IPMI request and print response
        i2c           Send an I2C Master Write-Read command and print response
        spd           Print SPD info from remote I2C device
        lan           Configure LAN Channels
        chassis       Get chassis status and set power state
        power         Shortcut to chassis power commands
        event         Send pre-defined events to MC
        mc            Management Controller status and global enables
        sdr           Print Sensor Data Repository entries and readings
        sensor        Print detailed sensor information
        fru           Print built-in FRU and scan SDR for FRU locators
        sel           Print System Event Log (SEL)
        pef           Configure Platform Event Filtering (PEF)
        sol           Configure and connect IPMIv2.0 Serial-over-LAN
        isol          Configure IPMIv1.5 Serial-over-LAN
        user          Configure Management Controller users
        channel       Configure Management Controller channels
        session       Print session information
        sunoem        OEM Commands for Sun servers
        kontronoem    OEM Commands for Kontron devices
        picmg         Run a PICMG/ATCA extended cmd
        fwum          Update IPMC using Kontron OEM Firmware Update Manager
        firewall      Configure Firmware Firewall
        exec          Run list of commands from file
        set           Set runtime variable for shell and exec
        hpm           Update HPM components using PICMG HPM.1 file
