
C:\Windows\Temp\Work2016\Utilities\ipmitool>ipmitool -i lan -h 192.168.7.45 -u r
oot -p superuser sel list
error in command line: Invalid argument
ipmitool version 1.8.14

usage: ipmitool [options...] <command>

       -h             This help
       -V             Show version information
       -v             Verbose (can use multiple times)
       -c             Display output in comma separated format
       -d N           Specify a /dev/ipmiN device to use (default=0)
       -I intf        Interface to use
       -H hostname    Remote host name for LAN interface
       -p port        Remote RMCP port [default=623]
       -U username    Remote session username
       -f file        Read remote session password from file
       -S sdr         Use local file for remote SDR cache
       -a             Prompt for remote password
       -e char        Set SOL escape character
       -C ciphersuite Cipher suite to be used by lanplus interface
       -k key         Use Kg key for IPMIv2 authentication
       -L level       Remote session privilege level [default=ADMINISTRATOR]
                      Append a '+' to use name/privilege lookup in RAKP1
       -A authtype    Force use of auth type NONE, PASSWORD, MD2, MD5 or OEM
       -P password    Remote session password
       -E             Read password from IPMI_PASSWORD environment variable
       -m address     Set local IPMB address
       -b channel     Set destination channel for bridged request
       -l lun         Set destination lun for raw commands
       -t address     Bridge request to remote target address
       -o oemtype     Setup for OEM (use 'list' to see available OEM types)
       -O seloem      Use file for OEM SEL event descriptions

Interfaces:
        imb           Intel IMB Interface [default]
        ism           SUN ISM Interface
        ms            Microsoft IPMI Interface
        lan           IPMI v1.5 LAN Interface
        lanplus       IPMI v2.0 RMCP+ LAN Interface

Commands:
        raw           Send a RAW IPMI request and print response
        i2c           Send an I2C Master Write-Read command and print response
        spd           Print SPD info from remote I2C device
        lan           Configure LAN Channels
        chassis       Get chassis status and set power state
        power         Shortcut to chassis power commands
        event         Send pre-defined events to MC
        mc            Management Controller status and global enables
        sdr           Print Sensor Data Repository entries and readings
        sensor        Print detailed sensor information
        fru           Print built-in FRU and scan SDR for FRU locators
        sel           Print System Event Log (SEL)
        pef           Configure Platform Event Filtering (PEF)
        sol           Configure and connect IPMIv2.0 Serial-over-LAN
        isol          Configure IPMIv1.5 Serial-over-LAN
        user          Configure Management Controller users
        channel       Configure Management Controller channels
        session       Print session information
        sunoem        OEM Commands for Sun servers
        kontronoem    OEM Commands for Kontron devices
        picmg         Run a PICMG/ATCA extended cmd
        fwum          Update IPMC using Kontron OEM Firmware Update Manager
        firewall      Configure Firmware Firewall
        exec          Run list of commands from file
        set           Set runtime variable for shell and exec
        hpm           Update HPM components using PICMG HPM.1 file


C:\Windows\Temp\Work2016\Utilities\ipmitool>