
g4Xflash:
------------------

Utility works using the Inband SCSI communication. User must have a valid/required drivers installed.


Limitations:
-------------------------------------------------

After performing "erase" operations on any of the active regions, user must perform the system power cycle. Otherwise, the erased regions will be continued to use as an Active region which may cause unknown behavior