*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG052033
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 3
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Sara Lee
* Approved By           : Ricky Lien
* RELEASE DATE          : 2021/01/22   (YYYY/MM/DD)
***************************************************************** 
HISTORY:
  1. [Fix #2266] BMC SEL event logged repeatedly by the removal and installation of PSU.
  2. [Fix #2272] The BMC Web displays incorrect fan information.
  3. [Fix #2279] The PSU Watt return value is "0" and PSU1&2 unable to detect the status.
  4. [Fix #2295] Even if the SEL log is full, no new events will be recorded.
  
*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG052032
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Mace Shen
* Approved By           : Ricky Lien
* RELEASE DATE          : 2020/11/13   (YYYY/MM/DD)
***************************************************************** 
HISTORY:
  1. [Fix #2237] Execute the "ipmitool sdr elist" command, FAN & PSU status return value is "NO Reading".
*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG012031
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 1
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Mace Shen
* Approved By           : Ricky Lien
* RELEASE DATE          : 2020/11/11   (YYYY/MM/DD)
***************************************************************** 
HISTORY:
  1. [Feature] Add BBU sensors.
  2. [Feature] BBU sensor show no reading, when BBU module not install.
*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011022
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 5
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Mace Shen
* Approved By           : Ricky Lien
* RELEASE DATE          : 2020/10/30   (YYYY/MM/DD)
***************************************************************** 
HISTORY:
	
  1. [Feature] Remove BBU sensors.
  2. [Feature] Modify the fan sensors to dual rotor fan.
  3. [Fixed #2117] The PRM value of fans doesn't rise up the speed when one of the fans is unplugged.
  4. [Fixed #2176] BMC sel displays unexpected event logs during AC test the beginning of the system booting.
  5. [Fixed] Removed one node that is higher PWM node, and the other node can't control SmartFan by itself.
  6. [Fixed] The external user services do not show on the WebUI setting page. 

*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011022
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 4
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Sara Lee
* Approved By           : Ricky Lien
* RELEASE DATE          : 2019/12/17   (YYYY/MM/DD)
*****************************************************************
HISTORY:
  
  1.[Fix][BUG #746] The BMC update with yafuflash under Linux is abnormal
  2.[Fix][BUG #789] The power button is no function after remote BIOS update with BMC via
  3.[Fix][BUG #790] Onboard NIC MAC address with X722 will be clear after remote bios update with BMC via(yafuflash).	

*****************************************************************
*			BMC firmware release note
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011022
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 3
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Julia Tsai
* Approved By           : Jack Hsu
* RELEASE DATE          : 2019/11/15   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1.[Fix] Fix BMC firmware update script.


NOTE:
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011022
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : Julia Tsai
* Approved By           : Jack Hsu
* RELEASE DATE          : 2019/11/13   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1.[Fix] Fix abnormal fan sensor event.
  2.[Fix] Fix show wrong BMC F/W version.
  3.[Fix] Fix show wrong fan sensor name on web gui.
  4.[Modify] Update sdr list file.
  5.[Modify] Optimize update script.
  6.[Add] Add AC lost event function.


NOTE:
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011022
* Firmware REV	        : VIRGM011
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 1
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : David Su
* Approved By           : Jack Hsu
* RELEASE DATE          : 2019/09/25   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1.[Feature] Modify fan sensor to single fan.


NOTE:
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011021
* Firmware REV	        : VIRGM011
* PMC REV               : SB403VG005001
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : David Su
* Approved By           : Jack Hsu
* RELEASE DATE          : 2019/09/5   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1.[Feature] Remove Fan_PCH, fix voltage reading abnormal issue..


NOTE:
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG011020
* Firmware REV	        : VIRGM011
* PMC REV               : SB403VG005001
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : David Su
* Approved By           : Jack Hsu
* RELEASE DATE          : 2018/09/18   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1.[Feature]Add BBU sensor.


NOTE:
*****************************************************************
* Platform              : HA401-VG
* BMC Config REV        : HA401VG010010
* Firmware REV	        : VIRGM010
* PMC REV               : SB403VG005001
* SDK REV               : 25r11.5_128366_171128_VIRGM005.tar.gz
* BMC CHIP              : AST2500
* Auxiliary REV         : 7
* NIC CHANNEL 1         : RTL8201EL-VC DEDICATED NIC
* NIC CHANNEL 8         : INTEL X772 SHARED NIC
* IPMI VER              : IPMI 2.0
* Engineer              : David Su
* Approved By           : Always Chen
* RELEASE DATE          : 2018/04/20   (YYYY/MM/DD)
*****************************************************************
HISTORY:

  1. First release for HA401-VG.


NOTE:
