AIC-PETv2-MIB DEFINITIONS ::= BEGIN
IMPORTS
    OBJECT-GROUP, MODULE-COMPLIANCE
        FROM SNMPv2-CONF
    MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, Integer32, Opaque, enterprises, snmpModules, IpAddress
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, DisplayString
        FROM SNMPv2-TC
	snmpTrap, system, snmpTrapEnterprise
		FROM SNMPv2-MIB;

aicPetMIB MODULE-IDENTITY
    LAST-UPDATED "202403200000Z"
    ORGANIZATION "AIC"
    CONTACT-INFO " "
    DESCRIPTION  "AIC BMC MIB for PET"
    REVISION     "202403200000Z"
    DESCRIPTION  "initial"
    ::= { snmpTrap 1  }

trapSpecific		OBJECT IDENTIFIER ::= { aicPetMIB 0 }
wiredformgmt    		OBJECT IDENTIFIER ::= { enterprises 3183 }
pet             		OBJECT IDENTIFIER ::= { wiredformgmt 1 }
petEvt			OBJECT IDENTIFIER ::= { pet 1 }
snmpCommunityMIB 		OBJECT IDENTIFIER ::= { snmpModules 18 }
snmpCommunityMIBObjects 	OBJECT IDENTIFIER ::= { snmpCommunityMIB 1 }
trapPefData		OBJECT IDENTIFIER ::= { petEvt 1 }

trapSensorDesc			OBJECT IDENTIFIER ::= {  petEvt 2 0 }

trapAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the agent-addr field of a Trap PDU which
         is forwarded by a proxy forwarder application using
         an SNMP version other than SNMPv1."
    ::= { snmpCommunityMIBObjects 3 }
	
trapCommunity OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the community string field of an SNMPv1
         message containing a Trap PDU which is forwarded by a
         a proxy forwarder application using an SNMP version
         other than SNMPv1."
    ::= { snmpCommunityMIBObjects 4 }

--trapSensorDesc OBJECT-TYPE
--    SYNTAX DisplayString
--    MAX-ACCESS accessible-for-notify
--    STATUS current
--    DESCRIPTION "Event Log"
--    ::= { petEvt 2 0}
	
trapUnderTemperatureWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Under-Temperature Warning (Lower non-critical, going low)"
    ::= { trapSpecific 65792 }

trapTemperatureRecoveredLNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Recovered (Lower non-critical, going high)"
    ::= { trapSpecific 65793 }

trapUnderTemperatureCritical NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Critical Under-Temperature Problem (Lower Critical - going low)"
    ::= { trapSpecific 65794 }

trapTemperatureLowWarningCritWarnLCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Temperature Low Warning: (Lower critical going high)."
    ::= { trapSpecific 65795 }

trapTemperatureLowCriticalCritNonRecoverLNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Temperature Low Critical (Lower non-recover going low)."
    ::= { trapSpecific 65796 }

trapTemperatureLowCriticalNonRecoverCritLNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Temperature Low Critical (Lower non-recover going high)."
    ::= { trapSpecific 65797 }

trapTemperatureRecoveredUNCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Recovered (Upper non-critical going low)"
    ::= { trapSpecific 65798 }

trapOverTemperatureWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Over-Temperature Warning (Upper non-critical, going high)"
    ::= { trapSpecific 65799 }

trapTempHighWarningCritWarnUCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Temperatur High Warning: (Upper critical going low)"
    ::= { trapSpecific 65800 }

trapOverTemperatureCritical NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Critical Over-Temperature Problem (Upper Critical - going high)"
    ::= { trapSpecific 65801 }

trapTempHighCriticalNonRecoverCritUNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Temperatur High Critical: (Upper non-recover going low)"
    ::= { trapSpecific 65802 }

trapTempHighCriticalCritNonRecoverUNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Temperatur High Critical: (Upper non-recover going high)"
    ::= { trapSpecific 65803 }

trapUnderTemperatureWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Under-Temperature Warning (Lower non-critical, going low) Cleared"
    ::= { trapSpecific 65920 }

trapTemperatureRecoveredLNCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Recovered (Lower non-critical, going high) Cleared"
    ::= { trapSpecific 65921 }

trapUnderTemperatureCriticalCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Critical Under-Temperature Problem (Lower Critical - going low) Cleared"
    ::= { trapSpecific 65922 }

trapTemperatureLowWarningCritWarnLCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Low Warning: (Lower critical going high) Cleared."
    ::= { trapSpecific 65923 }

trapTemperatureLowCriticalCritNonRecoverLNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Low Critical (Lower non-recover going low) Cleared."
    ::= { trapSpecific 65924 }

trapTemperatureLowCriticalNonRecoverCritLNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Low Critical (Lower non-recover going high) Cleared."
    ::= { trapSpecific 65925 }

trapTemperatureRecoveredUNCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperature Recovered (Upper non-critical going low)"
    ::= { trapSpecific 65926 }

trapOverTemperatureWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Over-Temperature warning Cleared"
    ::= { trapSpecific 65927 }

trapTempHighWarningCritWarnUCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperatur High Warning: (Upper critical going low) Cleared"
    ::= { trapSpecific 65928 }

trapOverTemperatureCriticalCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Critical Over-Temperature Problem (Upper Critical - going high)"
    ::= { trapSpecific 65929 }

trapTempHighCriticalNonRecoverCritUNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperatur High Critical: (Upper non-recover going low) Cleared"
    ::= { trapSpecific 65930 }

trapTempHighCriticalCritNonRecoverUNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Temperatur High Critical: (Upper non-recover going high) Cleared"
    ::= { trapSpecific 65931 }

trapGenericCriticalTemperature NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Generic Critical Temperature Problem (Transition to Critical from less severe)"
    ::= { trapSpecific 67330 }

trapGenericTemperatureWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Generic Temperature Warning (Transition to Warning from less severe)"
    ::= { trapSpecific 67331 }

trapUnderVoltageWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Under-Voltage Warning (Lower Non-Critical - going low)"
    ::= { trapSpecific 131328 }

trapVoltageRecoveredLNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Recovered (Lower non-critical, going high)"
    ::= { trapSpecific 131329 }

trapUnderVoltageCritical NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Critical Under-Voltage Problem (Lower Critical - going low)"
    ::= { trapSpecific 131330 }

trapVoltageLowNoLongerCriticalLCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Low - no longer Critical: (Lower critical going high)"
    ::= { trapSpecific 131331 }

trapVoltageLowCriticalCritNonRecoverLNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Voltage Low - Critical (Lower non-recover going low)"
    ::= { trapSpecific 131332 }

trapVoltageLowCriticalNonRecoverCritLNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Voltage Low - Critical (Lower non-recover going high)"
    ::= { trapSpecific 131333 }

trapVoltageRecoveredUNCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Recovered (Upper non critical going low)"
    ::= { trapSpecific 131334 }

trapOverVoltageWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Over-Voltage Warning (Upper Non-Critical - going high)"
    ::= { trapSpecific 131335 }

trapVoltageHighNoLongerCriticalUCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage High - no longer Critical: (Upper critical going low)"
    ::= { trapSpecific 131336 }

trapOverVoltageCritical NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Critical Over-Voltage Problem (Upper Critical - going high)"
    ::= { trapSpecific 131337 }

trapVoltageHighCriticalNonRecoverCritUNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Voltage High - Critical: (Upper non-recover going low)"
    ::= { trapSpecific 131338 }

trapVoltageHighCriticalCritNonRecoverUNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Voltage High - Critical: (Upper non-recover going high)"
    ::= { trapSpecific 131339 }

trapUnderVoltageWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Under-Voltage Warning Cleared"
    ::= { trapSpecific 131456 }

trapVoltageRecoveredLNCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Recovered (Lower non-critical, going high) Cleared"
    ::= { trapSpecific 131457 }


trapUnderVoltageCriticalCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Under-Voltage Problem Cleared"
    ::= { trapSpecific 131458 }

trapVoltageLowNoLongerCriticalLCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Low - no longer Critical: (Lower critical going high) Cleared"
    ::= { trapSpecific 131459 }

trapVoltageLowCriticalCritNonRecoverLNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Low - Critical (Lower non-recover going low) Cleared"
    ::= { trapSpecific 131460 }

trapVoltageLowCriticalNonRecoverCritLNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Low - Critical (Lower non-recover going high) Cleared"
    ::= { trapSpecific 131461 }

trapVoltageRecoveredUNCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage Recovered (Upper non critical going low) Cleared"
    ::= { trapSpecific 131462 }

trapOverVoltageWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Over-Voltage Warning Cleared"
    ::= { trapSpecific 131463 }

trapVoltageHighNoLongerCriticalUCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage High - no longer Critical: (Upper critical going low) Cleared"
    ::= { trapSpecific 131464 }

trapOverVoltageCriticalCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Over-Voltage Problem Cleared"
    ::= { trapSpecific 131465 }

trapVoltageHighCriticalNonRecoverCritUNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage High - Critical: (Upper non-recover going low) Cleared"
    ::= { trapSpecific 131466 }

trapVoltageHighCriticalCritNonRecoverUNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Voltage High - Critical: (Upper non-recover going high) Cleared"
    ::= { trapSpecific 131467 }

trapGenericCriticalDiscreteVoltageCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Generic Critical Voltage Problem Cleared"
    ::= { trapSpecific 131840 }

trapGenericCriticalDiscreteVoltage NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Generic Critical Voltage Problem (Transition to Critical from less severe)"
    ::= { trapSpecific 131841 }

trapGenericCriticalDiscreteVoltage2 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Generic Critical Voltage Problem (Transition to Critical from less severe)"
    ::= { trapSpecific 132866 }

trapGenericDiscreteVoltageWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Generic Voltage Warning (Transition to Non-Critical from less severe)"
    ::= { trapSpecific 132867 }

trapCurrentLowWarningLNCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Current Low Warning (Lower non critical going low)"
    ::= { trapSpecific 196864 }

trapCurrentRecoveredLNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Current Recovered (Lower non critical going high)"
    ::= { trapSpecific 196865 }

trapCurrentCriticalLowLCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current Critical Low (Lower critical going low)"
    ::= { trapSpecific 196866 }

trapCurrentNoLongerCriticalButLowLCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Current no longer Critical but Low (Lower critical going high)"
    ::= { trapSpecific 196867 }

trapCurrentLowDamageLNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current Low Damage (Lower non-recover going low)"
    ::= { trapSpecific 196868 }

trapCurrentNoLongerDamageButCriticalLowLNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current no longer Damage but Critical Low (Lower non-recover going high)"
    ::= { trapSpecific 196869 }

trapCurrentRecoveredUNCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Current Recovered (Upper non critical going low)"
    ::= { trapSpecific 196870 }

trapCurrentHighWarningUNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Current High Warning (Upper non critical going high)"
    ::= { trapSpecific 196871 }

trapCurrentNoLongerCriticalButHighUCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Current no longer Critical but High (Upper critical going low)"
    ::= { trapSpecific 196872 }

trapCurrentHighCriticalUCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current High Critical (Upper critical going high)"
    ::= { trapSpecific 196873 }

trapCurrentNoLongerDamageButCriticalHighUNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current no longer Damage but Critical High (Upper non-recover going low)"
    ::= { trapSpecific 196874 }

trapCurrentHighDamageUNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Current High Damage (Upper non-recover going high)"
    ::= { trapSpecific 196875 }

trapFanUnderSpeedWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Fan speed warning (Fan speed below expected speed)"
    ::= { trapSpecific 262400 }

trapFanIsWorkingOKLNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Recovered (Lower non critical going high)"
    ::= { trapSpecific 262401 }

trapFanCriticalUnderSpeed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Generic Critical Fan Failure (Transition to Critical from less severe)"
    ::= { trapSpecific 262402 }

trapFanPreFailCritWarnLCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Fan Pre-Fail: (Lower critical going high)"
    ::= { trapSpecific 262403 }

trapFanFailedCritNonRecoverLNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan Failed (Lower non-recover going low)"
    ::= { trapSpecific 262404 }

trapFanFailedNonRecoverCritLNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan Failed (Lower non-recover going high)"
    ::= { trapSpecific 262405 }

trapFanRecoveredUNCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Recovered (Upper non critical going low)"
    ::= { trapSpecific 262406 }

trapFanHighWarningUNCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Fan High Warning (Upper non critical going high)"
    ::= { trapSpecific 262407 }

trapFanNoLongerCriticalButHighUCGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan no longer Critical but High (Upper critical going low)"
    ::= { trapSpecific 262408 }

trapFanHighCriticalUCGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan High Critical (Upper critical going high)"
    ::= { trapSpecific 262409 }

trapFanNoLongerDamageButCriticalHighUNRGL NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan no longer Damage but Critical High (Upper non-recover going low)"
    ::= { trapSpecific 262410 }

trapFanHighDamageUNRGH NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan High Damage (Upper non-recover going high)"
    ::= { trapSpecific 262411 }

trapFanUnderSpeedWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan speed Warning Cleared"
    ::= { trapSpecific 262528 }

trapFanIsWorkingOKLNCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Recovered (Lower non critical going high) Cleared"
    ::= { trapSpecific 262529 }

trapFanCriticalUnderSpeedCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Critical Fan Failure Cleared"
    ::= { trapSpecific 262530 }

trapFanPreFailCritWarnLCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Pre-Fail: (Lower critical going high) Cleared"
    ::= { trapSpecific 262531 }

trapFanFailedCritNonRecoverLNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Failed (Lower non-recover going low) Cleared"
    ::= { trapSpecific 262532 }

trapFanFailedNonRecoverCritLNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Failed (Lower non-recover going high) Cleared"
    ::= { trapSpecific 262533 }

trapFanRecoveredUNCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan Recovered (Upper non critical going low) Cleared"
    ::= { trapSpecific 262534 }

trapFanHighWarningUNCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan High Warning (Upper non critical going high) Cleared"
    ::= { trapSpecific 262535 }

trapFanNoLongerCriticalButHighUCGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan no longer Critical but High (Upper critical going low) Cleared"
    ::= { trapSpecific 262536 }

trapFanHighCriticalUCGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan High Critical (Upper critical going high) Cleared"
    ::= { trapSpecific 262537 }

trapFanNoLongerDamageButCriticalHighUNRGLCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan no longer Damage but Critical High (Upper non-recover going low) Cleared"
    ::= { trapSpecific 262538 }

trapFanHighDamageUNRGHCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan High Damage (Upper non-recover going high) Cleared"
    ::= { trapSpecific 262539 }

trapFanFullRedundancy NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Fan redundancy has returned to Normal"
    ::= { trapSpecific 264960 }

trapFanRedundancyLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fan Redundancy has been Lost"
    ::= { trapSpecific 264961 }

trapFanRedundancyDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Fan Redundancy is in a degraded state"
    ::= { trapSpecific 264962 }

trapPowerSupplyFullRedundancy NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply Redundancy Has Returned to Normal"
    ::= { trapSpecific 527104 }

trapPowerSupplyRedundancyLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Supply Redundancy has been Lost"
    ::= { trapSpecific 527105 }

trapPowerSupplyRedundancyDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Supply Redundancy is in a degraded state"
    ::= { trapSpecific 527106 }

trapPowerUnitRedundancyOk NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Unit Redundancy has been restored"
    ::= { trapSpecific 592640 }

trapPowerUnitRedundancyLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Unit Redundancy has been Lost"
    ::= { trapSpecific 592641 }

trapOEMTransitionToIdle NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to idle"
    ::= { trapSpecific 12583424 }

trapOEMTransitionToActive NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to active"
    ::= { trapSpecific 12583425 }

trapOEMTransitionToBusy NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to busy"
    ::= { trapSpecific 12583426 }

trapOEMStateDeasserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] state deasserted"
    ::= { trapSpecific 12583680 }

trapOEMStateAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] state asserted"
    ::= { trapSpecific 12583681 }

trapOEMPredictiveFailureDeasserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] predictive failure deasserted"
    ::= { trapSpecific 12583936 }

trapOEMPredictiveFailureAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] predictive failure asserted"
    ::= { trapSpecific 12583937 }

trapOEMLimitNotExceeded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] limit not exceeded"
    ::= { trapSpecific 12584192 }

trapOEMLimitExceeded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] limit exceeded"
    ::= { trapSpecific 12584193 }

trapOEMPerformanceMet NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] performance met"
    ::= { trapSpecific 12584448 }

trapOEMPerformanceLags NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] performance lags"
    ::= { trapSpecific 12584449 }

trapOEMTransitionToOk NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to ok"
    ::= { trapSpecific 12584704 }

trapOEMTransitionToNonCriticalFromOk NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] transition to non critical from ok"
    ::= { trapSpecific 12584705 }

trapOEMTransitionToCriticalFromLessSevere NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] transition to critical from less severe"
    ::= { trapSpecific 12584706 }

trapOEMTransitionToNonRecoverableFromLessSevere NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] transition to non recoverable from less severe"
    ::= { trapSpecific 12584707 }

trapOEMTransitionToNonCriticalFromMoreSevere NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] transition to non critical from more severe"
    ::= { trapSpecific 12584708 }

trapOEMTransitionToCriticalFromNonRecoverable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] transition to critical from non recoverable"
    ::= { trapSpecific 12584709 }

trapOEMTransitionToNonRecoverable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] transition to non recoverable"
    ::= { trapSpecific 12584710 }

trapOEMMonitor NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] monitor"
    ::= { trapSpecific 12584711 }

trapOEMInformational NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] informational"
    ::= { trapSpecific 12584712 }

trapOEMDeviceRemovedDeviceAbsent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] device removed device absent"
    ::= { trapSpecific 12584960 }

trapOEMDeviceInsertedDdevicePresent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] device inserted device present"
    ::= { trapSpecific 12584961 }

trapOEMDeviceDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] device disabled"
    ::= { trapSpecific 12585216 }

trapOEMDeviceEnabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] device enabled"
    ::= { trapSpecific 12585217 }

trapOEMTransitionTorRunning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to rRunning"
    ::= { trapSpecific 12585472 }

trapOEMTransitionToInTest NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to in test"
    ::= { trapSpecific 12585473 }

trapOEMTransitionToPowerOff NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to power off"
    ::= { trapSpecific 12585474 }

trapOEMTransitionToOnLine NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to on line"
    ::= { trapSpecific 12585475 }

trapOEMTransitionToOffLine NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to off line"
    ::= { trapSpecific 12585476 }

trapOEMTransitionToOffDuty NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to off duty"
    ::= { trapSpecific 12585477 }

trapOEMTransitionToDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] transition to degraded"
    ::= { trapSpecific 12585478 }

trapOEMTransitionToPowerSave NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] transition to power save"
    ::= { trapSpecific 12585479 }

trapOEMInstallError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] install error"
    ::= { trapSpecific 12585480 }

trapOEMFullyRedundantRedundancyRegained NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] fully redundant redundancy regained"
    ::= { trapSpecific 12585728 }

trapOEMRedundancyLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] redundancy lost"
    ::= { trapSpecific 12585729 }

trapOEMRedundancyDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] redundancy degraded"
    ::= { trapSpecific 12585730 }

trapOEMNonRedundantSufficientResourcesFromRedundant NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] non redundant sufficient resources from redundant"
    ::= { trapSpecific 12585731 }

trapOEMNonRedundantSufficientResourcesFromInsufficientResources NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] non redundant sufficient resources from insufficient resources"
    ::= { trapSpecific 12585732 }

trapOEMNonRedundantInsufficientResources NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] non redundant insufficient resources"
    ::= { trapSpecific 12585733 }

trapOEMRedundancyDegradedFromFullyRedundant NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] redundancy degraded from fully redundant"
    ::= { trapSpecific 12585734 }

trapOEMRedundancyDegradedFromNonRedundant NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] redundancy degraded from non redundant"
    ::= { trapSpecific 12585735 }

trapOEMD0PowerState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] d0 power state"
    ::= { trapSpecific 12585984 }

trapOEMD1PowerState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] d1 power state"
    ::= { trapSpecific 12585985 }

trapOEMD2PowerState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] d2 power state"
    ::= { trapSpecific 12585986 }

trapOEMD3PowerState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] d3 power state"
    ::= { trapSpecific 12585987 }

trapChassisIntrusion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Chassis Open"
    ::= { trapSpecific 356096 }

trapDriveBayIntrusion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Drive Bay Open"
    ::= { trapSpecific 356097 }

trapIOAreaIntrusion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] I/O Card Area Open"
    ::= { trapSpecific 356098 }

trapProcessorAreaIntrusion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Processor Area Open"
    ::= { trapSpecific 356099 }

trapLANDisconnect NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] LAN Disconnected"
    ::= { trapSpecific 356100 }

trapUnautorizedDock NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Docking Permission Deasserted"
    ::= { trapSpecific 356101 }

trapFANAreaIntrusion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] FAN Area Open"
    ::= { trapSpecific 356102 }

trapChassisIntrusionClosed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Chassis Closed"
    ::= { trapSpecific 356224 }

trapSecureModeViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Secure Mode Violation"
    ::= { trapSpecific 421632 }

trapPrebootUserPasswordViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Pre-boot User password violation"
    ::= { trapSpecific 421633 }

trapPrebootSetupPasswordViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Pre-boot Setup password violation"
    ::= { trapSpecific 421634 }

trapNetworkBootPasswordViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Network Boot Password Violation"
    ::= { trapSpecific 421635 }

trapPasswordViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Password Violation"
    ::= { trapSpecific 421636 }

trapOutOfBandPasswordViolation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Out-of-band Password Violation"
    ::= { trapSpecific 421637 }

trapProcessorInternalError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Processor Internal Error"
    ::= { trapSpecific 487168 }

trapProcessorThermalTrip NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Over Temperature Condition Detected for Processor)"
    ::= { trapSpecific 487169 }

trapProcessorBistError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Processor Failed - FRB1/BIST"
    ::= { trapSpecific 487170 }

trapProcessorFRB2Failure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Processor Failed - FRB2/POST"
    ::= { trapSpecific 487171 }

trapProcessorFRB3Failure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Processor Failed - FRB3"
    ::= { trapSpecific 487172 }

trapProcessorConfigError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Processor Configuration Mismatch"
    ::= { trapSpecific 487173 }

trapSMBIOSUncorrectableCPUComplexError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] SMBIOS Uncorrectable CPU Complex Error asserted"
    ::= { trapSpecific 487174 }

trapProcessorAdded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Added"
    ::= { trapSpecific 487175 }

trapCPUDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] CPU Disabled"
    ::= { trapSpecific 487176 }

trapProcessorTerminatorDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Terminator Detected"
    ::= { trapSpecific 487177 }

trapProcessorThrottle NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Processor Degraded"
    ::= { trapSpecific 487178 }

trapMachineCheckExceptionUncorrectable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Machine Check Exception"
    ::= { trapSpecific 487179 }

trapCorrectableMachineCheckError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Correctable Machine Check Error"
    ::= { trapSpecific 487180 }

trapProcessorInternalErrorCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Internal Error Cleared"
    ::= { trapSpecific 487296 }

trapProcessorThermalTripCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Over Temperature Condition Removed for Processor"
    ::= { trapSpecific 487297 }

trapProcessorBistErrorCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Recovered from FRB1/BIST"
    ::= { trapSpecific 487298 }

trapProcessorConfigErrorCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Recovered - Configuration Mismatch"
    ::= { trapSpecific 487301 }

trapProcessorThrottleCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Processor Not Degraded"
    ::= { trapSpecific 487306 }

trapPowerSupplyPresenceDeteced NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply Inserted"
    ::= { trapSpecific 552704 }

trapPowerSupplyFailureDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power supply Failure detected"
    ::= { trapSpecific 552705 }

trapPowerSupplyWarning NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power supply Warning"
    ::= { trapSpecific 552706 }

trapPowerSupplyACLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Supply AC Lost"
    ::= { trapSpecific 552707 }

trapPowerSupplyInputLostOrOutOfRange NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Supply input lost or out of range"
    ::= { trapSpecific 552708 }


trapPowerSupplyInputOutOfRange NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Supply input out of range"
    ::= { trapSpecific 552709 }

trapPowerSupplyConfigurationError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Supply Configuration Error"
    ::= { trapSpecific 552710 }

trapPowerSupplyPresenceRemoved NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Supply Removed"
    ::= { trapSpecific 552832 }

trapPowerSupplyFailureCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply Failure Cleared"
    ::= { trapSpecific 552833 }

trapPowerSupplyWarningCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply Warning Cleared"
    ::= { trapSpecific 552834 }

trapPowerSupplyACBack NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= { trapSpecific 552835 }

trapPowerSupplyInputOKOrWithinRange NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= { trapSpecific 552836 }

trapPowerSupplyInputOKfromOutofrange NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= { trapSpecific 552837 }

trapPowerSupplyConfigOK NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Supply configuration is OK"
    ::= { trapSpecific 552838 }

trapPowerUnitPowerOffPowerDown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Unit Disabled"
    ::= { trapSpecific 618240 }

trapPowerUnitPowerCycleAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Unit power cycled"
    ::= { trapSpecific 618241 }

trapPowerUnit240VAPowerDown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Unit 240VA power down error"
    ::= { trapSpecific 618242 }

trapInterlockPowerDown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Unit Interlock power down error"
    ::= { trapSpecific 618243 }

trapPowerUnitACLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Power Unit power lost"
    ::= { trapSpecific 618244 }

trapPowerUnitSoftPowerControlFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Unit soft power control failed"
    ::= { trapSpecific 618245 }

trapPowerUnitFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Unit failed"
    ::= { trapSpecific 618246 }

trapPowerUnitPredictiveFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Power Unit Predictive Failure"
    ::= { trapSpecific 618247 }

trapMemoryCorrectableECC NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Memory Corrected Error Detected"
    ::= { trapSpecific 814848 }

trapMemoryUncorrectableECC NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Memory uncorrectable error detected"
    ::= { trapSpecific 814849 }

trapMemoryParityError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Memory Parity Error Detected"
    ::= { trapSpecific 814850 }

trapMemoryScrubFailed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Memory Scrub Failure"
    ::= { trapSpecific 814851 }

trapMemoryDeviceDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Memory Disabled"
    ::= { trapSpecific 814852 }

trapMemoryECCLoggingLimitReached NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Memory Logging Limit Reached"
    ::= { trapSpecific 814853 }

trapMemoryPresenceDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Memory Added"
    ::= { trapSpecific 814854 }

trapMemoryConfigurationError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Memory DIMM Configuration Error"
    ::= { trapSpecific 814855 }

trapMemorySpare NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Memory double chip sparing initiated"
    ::= { trapSpecific 814856 }

trapMemoryThrottled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Memory Throttled"
    ::= { trapSpecific 814857 }

trapMemoryCriticalOvertemperature NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Over Temperature Condition Detected for Memory"
    ::= { trapSpecific 814858 }

trapDriveDriveAdded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Drive Added"
    ::= { trapSpecific 880384 }

trapDriveDriveFault NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Drive Disabled due to fault"
    ::= { trapSpecific 880385 }

trapDrivePredictiveFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Array Failure Predicted"
    ::= { trapSpecific 880386 }

trapDriveHotSpare NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Hot Spare Enabled"
    ::= { trapSpecific 880387 }

trapDriveConsistencyCheckInProgress NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Consistency Check Begun"
    ::= { trapSpecific 880388 }

trapDriveInCriticalArray NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Array Critical"
    ::= { trapSpecific 880389 }

trapDriveInFailedArray NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Failed Array"
    ::= { trapSpecific 880390 }

trapDriveRebuildRemapInProgress NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Rebuild in Progress"
    ::= { trapSpecific 880391 }

trapDriveRebuildRemapAbortedwasNotCompletedNormally NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Rebuild Aborted"
    ::= { trapSpecific 880392 }

trapPostError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Post Error"
    ::= { trapSpecific 1011456 }

trapSystemFirmwareHang NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] System Firmware Hang"
    ::= { trapSpecific 1011457 }

trapSystemFirmwareProgress NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System Firmware Progress"
    ::= { trapSpecific 1011458 }

trapCorrectableMemoryErrorLoggingDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Memory Logging Disabled"
    ::= { trapSpecific 1076992 }

trapEventLoggingDisablede NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Event Logging Disabled"
    ::= { trapSpecific 1076993 }

trapLogCleared NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Log Cleared"
    ::= { trapSpecific 1076994 }

trapAllEventLoggingDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] All Event Logging Disabled"
    ::= { trapSpecific 1076995 }

trapLogFull NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Log Full"
    ::= { trapSpecific 1076996 }

trapLogAlmostFull NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Log Almost Full"
    ::= { trapSpecific 1076997 }

trapCorrectableMachineCheckErrorLoggingDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Correctable Machine Check Error Logging Disabled"
    ::= { trapSpecific 1076998 }

trapBIOSWatchdogReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] BIOS Watchdog Reset"
    ::= { trapSpecific 1142528 }

trapOSWatchdogReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog Reset"
    ::= { trapSpecific 1142529 }

trapOSWatchdogShutdown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog Shutdown"
    ::= { trapSpecific 1142530 }

trapOSWatchdogPowerDown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog Power Down"
    ::= { trapSpecific 1142531 }

trapOSWatchdogPowerCycle NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog Power Cycle"
    ::= { trapSpecific 1142532 }

trapOSWatchdogNMIDiagnosticInterrupt NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog NMI / Diagnostic Interrupt"
    ::= { trapSpecific 1142533 }

trapOSWatchdogExpired NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] OS Watchdog Expired, status only"
    ::= { trapSpecific 1142534 }

trapOSWatchdogPretimeoutInterruptNonNMI NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] OS Watchdog pre-timeout Interrupt, non-NMI"
    ::= { trapSpecific 1142535 }

trapSystemReconfigured NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] System Reconfigured"
    ::= { trapSpecific 1208064 }

trapOEMSystemBootEvent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] OEM System Boot Event"
    ::= { trapSpecific 1208065 }

trapUnknownSystemHardwareFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Unknown System Hardware Failure"
    ::= { trapSpecific 1208066 }

trapAuxiliaryLogEntryEvent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Auxiliary Log Entry Event"
    ::= { trapSpecific 1208067 }

trapPEFActionExecuted NOTIFICATION-TYPE
	 STATUS 	 current
	 DESCRIPTION
	   "A traffic event trap."
	 ::={trapSpecific 1208068}

trapTimestampClockSynch NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Timestamp Clock Synch"
    ::= { trapSpecific 1208069 }

trapFrontPanelNMIDiagnosticInterrupt NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Front Panel NMI / Diagnostic Interrupt"
    ::= { trapSpecific 1273600 }

trapBusTimeout NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Bus Timeout"
    ::= { trapSpecific 1273601 }

trapIOChannelNMI NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] IO Channel check NMI"
    ::= { trapSpecific 1273602 }

trapSoftwareNMI NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] software NMI"
    ::= { trapSpecific 1273603 }

trapPCIPERR NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] PCI PERR"
    ::= { trapSpecific 1273604 }

trapPCISERR NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] PCI SERR"
    ::= { trapSpecific 1273605 }

trapBusUncorrectError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Bus Uncorrectable Error"
    ::= { trapSpecific 1273608 }

trapFatalNMI NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Fatal NMI"
    ::= { trapSpecific 1273609 }

trapBusFatalError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Bus Fatal Error"
    ::= { trapSpecific 1273610 }

trapBusDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Bus Degraded"
    ::= { trapSpecific 1273611 }

trapPowerButtonPressed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Power Button pressed"
    ::= { trapSpecific 1339136 }

trapSleepButtonPressed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Sleep Button pressed"
    ::= { trapSpecific 1339137 }

trapResetButtonPressed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Reset Button pressed"
    ::= { trapSpecific 1339138 }

trapFRULatchOpen NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU latch open"
    ::= { trapSpecific 1339139 }

trapFRUServiceRequestButton NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU service request button"
    ::= { trapSpecific 1339140 }

trapChassisPowerOnAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Chassis Transition to Running - Asserted"
    ::= { trapSpecific 1575424 }

trapChassisPowerOffAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Chassis Transition to Power Off - Asserted"
    ::= { trapSpecific 1575426 }


trapSoftPowerControlFailed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Soft Power Control Failed"
    ::= { trapSpecific 1666816 }

trapThermalTrip NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Thermal trip"
    ::= { trapSpecific 1666817 }

trapCableInterconnectIsConnected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Cable Interconnect is connected"
    ::= { trapSpecific 1798016 }

trapConfigurationError NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Configuration Error - Incorrect cable connected / Incorrect interconnection"
    ::= { trapSpecific 1798017 }

trapSystemInitiatedByPowerUp NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System Initiated by PowerUp"
    ::= { trapSpecific 1928960 }

trapSystemInitiatedByHardReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System Initiated by Hard Reset"
    ::= { trapSpecific 1928961 }

trapSystemInitiatedByWarmReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System Initiated by Warm Reset"
    ::= { trapSpecific 1928962 }

trapUserRequestedPXEBoot NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] User requested PXE boot"
    ::= { trapSpecific 1928963 }

trapAutomaticBootToDiagnostic NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Automatic boot to diagnostic"
    ::= { trapSpecific 1928964 }

trapOSRuntimeSoftwareInitiatedHardReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] OS / runtime software initiated hard Reset"
    ::= { trapSpecific 1928965 }

trapOSRuntimeSoftwareInitiatedWarmReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] OS / runtime software initiated warm Reset"
    ::= { trapSpecific 1928966 }

trapSystemRestart NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System Restart"
    ::= { trapSpecific 1928967 }

trapNoBootableMedia NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] No bootable media"
    ::= { trapSpecific 1994496 }

trapNonBootableDisketteLeftInDrive NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Non bootable diskette left in drive"
    ::= { trapSpecific 1994497 }

trapPXEServerNotFound NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] PXE Server not found"
    ::= { trapSpecific 1994498 }

trapInvalidBootSector NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Invalid boot sector"
    ::= { trapSpecific 1994499 }

trapTimeoutWaitingForUserSelectionOfBootSource NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Timeout waiting for user selection of boot source"
    ::= { trapSpecific 1994500 }

trapABootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] A: Boot completed"
    ::= { trapSpecific 2060032 }

trapCBootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] C: Boot completed"
    ::= { trapSpecific 2060033 }

trapPXEBootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] PXE Boot completed"
    ::= { trapSpecific 2060034 }

trapDiagnosticBootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Diagnostic Boot completed"
    ::= { trapSpecific 2060035 }

trapCDROMBootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] CD-ROM Boot completed"
    ::= { trapSpecific 2060036 }

trapROMBootCompleted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] ROM Boot completed"
    ::= { trapSpecific 2060037 }

trapBootCompletedBootDeviceNotSpecified NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Boot completed - boot device not specified"
    ::= { trapSpecific 2060038 }

trapStopDuringOSLoadInitialization NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Stop during OS load / initialization"
    ::= { trapSpecific 2125568 }

trapRuntimeStop NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Run-time Stop"
    ::= { trapSpecific 2125569 }

trapOSGracefulCriticalStop NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] OS Graceful Critical Stop"
    ::= { trapSpecific 2125570 }

trapOSGracefulShutdown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] OS Graceful Shutdown"
    ::= { trapSpecific 2125571 }

trapSoftShutdownInitiatedByPEF NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Soft Shutdown initiated by PEF"
    ::= { trapSpecific 2125572 }

trapAgentNotResponding NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Agent Not Responding"
    ::= { trapSpecific 2125573 }

trapSlotFaultAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Fault Status asserted"
    ::= { trapSpecific 2191104 }

trapSlotIdentifyAsserted NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Identify Status asserted"
    ::= { trapSpecific 2191105 }

trapSlotDeviceInstalled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot / Connector Device installed/attached"
    ::= { trapSpecific 2191106 }

trapSlotReadyForDeviceInstallation NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot / Connector Ready for Device Installation"
    ::= { trapSpecific 2191107 }

trapSlotReadyForDeviceRemoval NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot/Connector Ready for Device Removal"
    ::= { trapSpecific 2191108 }

trapSlotPoweredOff NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot Power is Off"
    ::= { trapSpecific 2191109 }

trapSlotRemovalRequest NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot / Connector Device Removal Request"
    ::= { trapSpecific 2191110 }

trapSlotInterlockAssertedlatchNotClosed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Interlock asserted"
    ::= { trapSpecific 2191111 }

trapSlotDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot is Disabled"
    ::= { trapSpecific 2191112 }

trapSlotHoldsSpareDevice NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Slot holds spare device"
    ::= { trapSpecific 2191113 }

trapSystemACPIPowerStateWorkingS0G0 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S0 / G0 working"
    ::= { trapSpecific 2256640 }

trapSystemACPIPowerStateSleepingS1 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S1 sleeping"
    ::= { trapSpecific 2256641 }

trapSystemACPIPowerStateSleepingS2 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S2 sleeping, processor context lost"
    ::= { trapSpecific 2256642 }

trapSystemACPIPowerStateSleepingS3 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S3 sleeping, processor & h/w context lost, memory retained"
    ::= { trapSpecific 2256643 }

trapSystemACPIPowerStateSleepingS4SuspendToDisk NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S4 non-volatile sleep / suspend-to disk"
    ::= { trapSpecific 2256644 }

trapSystemACPIPowerStateSleepingS5SoftOff NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S5 / G2 soft-off"
    ::= { trapSpecific 2256645 }

trapSystemACPIPowerStateSleepingS4S5 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S4 / S5 soft-off, particular S4 / S5 state cannot be determined"
    ::= { trapSpecific 2256646 }

trapSystemACPIPowerStateSleepingG7MechanicalOff NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] G3 / Mechanical Off"
    ::= { trapSpecific 2256647 }

trapSystemACPIPowerStateSleepingS1S2S3 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Sleeping in an S1, S2, or S3 states"
    ::= { trapSpecific 2256648 }

trapSystemACPIPowerStateSleepingG1 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] G1 sleeping"
    ::= { trapSpecific 2256649 }

trapSystemACPIPowerStateSleepingS5ByOverrride NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] S5 entered by override"
    ::= { trapSpecific 2256650 }

trapSystemACPIPowerStateLegacyONState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Legacy ON State"
    ::= { trapSpecific 2256651 }

trapSystemACPIPowerStateLegacyOFFState NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Legacy OFF State"
    ::= { trapSpecific 2256652 }

trapSystemACPIPowerStateInvalid NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System ACPI Power State Invalid"
    ::= { trapSpecific 2256653 }

trapSystemACPIPowerStateUnknown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] System ACPI Power State Unknown"
    ::= { trapSpecific 2256654 }

trapWatchdogTimerExpired NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Timer expired, status only"
    ::= { trapSpecific 2322176 }

trapWatchdogHardReset NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Hard Reset"
    ::= { trapSpecific 2322177 }

trapWatchdogPowerDown NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Power Down"
    ::= { trapSpecific 2322178 }

trapWatchdogPowerCycle NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Power Cycle"
    ::= { trapSpecific 2322179 }

trapWatchdogHardwareWatchdogExpired NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Hardware Watchdog expired"
    ::= { trapSpecific 2322180 }

trapWatchdogTimerInterrupt NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Watchdog Timer Interrupt"
    ::= { trapSpecific 2322184 }

trapPlatformAlertGeneratedPage NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] platform generated page"
    ::= { trapSpecific 2387712 }

trapPlatformAlertGeneratedLANAlert NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] platform generated LAN alert"
    ::= { trapSpecific 2387713 }

trapPlatformAlertEventTrapGenerated NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Platform Event Trap generated, formatted per IPMI PET specification"
    ::= { trapSpecific 2387714 }

trapPlatformAlertGeneratedSNMPTrap NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] platform generated SNMP trap, OEM format"
    ::= { trapSpecific 2387715 }

trapEntityPresent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Entity Present"
    ::= { trapSpecific 2453248 }

trapEntityAbsent NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Entity Absent"
    ::= { trapSpecific 2453249 }

trapEntityDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Entity Disabled"
    ::= { trapSpecific 2453250 }

trapLANHeartbeatLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] LAN Heartbeat Lost"
    ::= { trapSpecific 2584320 }

trapLANHeartbeat NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] LAN Heartbeat"
    ::= { trapSpecific 2584321 }

trapSensorAccessDegraded NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] sensor access degraded or unavailable"
    ::= { trapSpecific 2649856 }

trapControllerAccessDegradedOrUnavailable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Controller access degraded or unavailable"
    ::= { trapSpecific 2649857 }

trapManagementControllerOffline NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Management Controller off-line"
    ::= { trapSpecific 2649858 }

trapManagementControllerUnavailable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Critical] Management Controller unavailable"
    ::= { trapSpecific 2649859 }

trapSensorFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Sensor Failure"
    ::= { trapSpecific 2649860 }

trapFRUFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] FRU Failure"
    ::= { trapSpecific 2649861 }

trapBatteryLowpredictiveFailure NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Battery low (predictive failure)"
    ::= { trapSpecific 2715392 }

trapBatteryFailed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Battery failed"
    ::= { trapSpecific 2715393 }

trapBatteryPresenceDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Battery presence detected"
    ::= { trapSpecific 2715394 }

trapSessionActivated NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Session Activated"
    ::= { trapSpecific 2780928 }

trapSessionDeactivated NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Session Deactivated"
    ::= { trapSpecific 2780929 }

trapInvalidUsernameOrPassword NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Invalid Username or Password"
    ::= { trapSpecific 2780930 }

trapInvalidPasswordDisable NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Invalid password disable"
    ::= { trapSpecific 2780931 }

trapHWChangeDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Hardware change detected with associated Entity"
    ::= { trapSpecific 2846464 }

trapFWOrSWChangeDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Firmware or software change detected with associated Entity"
    ::= { trapSpecific 2846465 }

trapHWIncompatibilityDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Hardware incompatibility detected with associated Entity"
    ::= { trapSpecific 2846466 }

trapFWOrSWIncompatibilityDetected NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Firmware or software incompatibility detected with associated Entity"
    ::= { trapSpecific 2846467 }

trapInvalidUnsupportedHWVersion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Entity is of an invalid or unsupported hardware version"
    ::= { trapSpecific 2846468 }

trapInvalidUnsupportedFWOrSWVersion NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Entity contains an invalid or unsupported firmware or software version"
    ::= { trapSpecific 2846469 }

trapHWChangeSuccessful NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Hardware Change detected with associated Entity was successful"
    ::= { trapSpecific 2846470 }

trapSWOrFWChangeSuccessful NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] Software or F/W Change detected with associated Entity was successful"
    ::= { trapSpecific 2846471 }

trapFRUNotInstalled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] FRU Not Installed"
    ::= { trapSpecific 2912000 }

trapFRUInactive NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] FRU Inactive"
    ::= { trapSpecific 2912001 }

trapFRUActivationRequested NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU Activation Requested"
    ::= { trapSpecific 2912002 }

trapFRUActivationInProgress NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU Activation In Progress"
    ::= { trapSpecific 2912003 }

trapFRUActive NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU active"
    ::= { trapSpecific 2912004 }

trapFRUDeactivationRequested NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU Deactivation Requested"
    ::= { trapSpecific 2912005 }

trapFRUDeactivationInProgress NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Informational] FRU Deactivation In Progress"
    ::= { trapSpecific 2912006 }

trapFRUConnectionLost NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] FRU Communication Lost"
    ::= { trapSpecific 2912007 }

trapOEMSpecific NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] OEM Specific"
    ::= { trapSpecific 12611328 }

trapTransitionToM0 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M0"
    ::= { trapSpecific 15757056 }

trapTransitionToM1 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M1"
    ::= { trapSpecific 15757057 }

trapTransitionToM2 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M2"
    ::= { trapSpecific 15757058 }

trapTransitionToM3 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M3"
    ::= { trapSpecific 15757059 }

trapTransitionToM4 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M4"
    ::= { trapSpecific 15757060 }

trapTransitionToM5 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M5"
    ::= { trapSpecific 15757061 }

trapTransitionToM6 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M6"
    ::= { trapSpecific 15757062 }

trapTransitionToM7 NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Transition to M7"
    ::= { trapSpecific 15757063 }

trapIPMBAdisabledIPMBBDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] IPMB A disabled IPMB B disabled"
    ::= { trapSpecific 15822592 }

trapIPMBAenabledIPMBBDisabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] IPMB A enabled IPMB B disabled"
    ::= { trapSpecific 15822593 }

trapIPMBAdisabledIPMBBEnabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] IPMB A disabled IPMB B enabled"
    ::= { trapSpecific 15822594 }

trapIPMBAenabledIPMBBEnabled NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] IPMB A enabled IPMB B enabled"
    ::= { trapSpecific 15822595 }

trapModuleHandleClosed NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Module handle closed"
    ::= { trapSpecific 15888128 }

trapModuleHandleOpened NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Module handle opened"
    ::= { trapSpecific 15888129 }


trapQuiesced NOTIFICATION-TYPE
    STATUS current
    DESCRIPTION "[Warning] Quiesced"
    ::= { trapSpecific 15888130 }

END
