*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC010802
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 17ef79286c85c2d733cf1f5e1cbb0b37858905f5
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/06/13   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Implement PSU_Watt sensor for each PSU.
    2. [Feature] Implement PSU_Voltage sensor for each PSU.
    3. [Feature] Implement PSU_Temp sensor for each PSU.
    4. [Feature] [Web] Implement PSU Health statuses.
    5. [Feature] [Web] Implement manual fan control on web.
    6. [Feature] [Redfish] Implement PSU FW version, Model, LineInputVoltage, PowerInputWatts and Status in Redfish.
    7. [Feature] [Redfish] Support fan mode via redfish interface.
    8. [Fixed #9012] BMC Web interface does not have a PSU Information page.
    9. [Fixed #9035] After entering the OEM command in the system, there is no action.
    10. [Fixed #9639] There are missing some sensor on SDR-List.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. Due to SDR changed, do not preserve configuration when update BMC firmware.
    4. Use BIOS version TUCH0070 or above.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC000702
* GIT repository        : ami_lts_v12_update_3
* GIT version           : c002e3512e835d41ae2ae6ecd286de8e6518e2b9
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/05/29   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Fix] Web inventory page PCIe device location is duplicated.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. This is a beta version.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC010702
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 9d6374d10e4c22a1453b627ebaea9457305c0adf
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/03/28   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Update Product ID to 3061.

Note:
    1. The first four byte "3060" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : 3060TUC011002
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 2d1296a24e312b53813179573bd3314276c9c360
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/03/13   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Moniter DIMM throttled after BOM boot complete.
    2. [Feature] Implement setting for KVM never timeout.
    3. [Fixed #8999] SDR list lacks clear classification and definition.

Note:
    1. The first four byte "3060" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : 3060TUC010902
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 50ee96e688791945553ae3aa38b2f0bc5e8e9206
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/02/20   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Update Product ID to 3060.

Note:
    1. The first four byte "3060" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC010602
* GIT repository        : ami_lts_v12_update_3
* GIT version           : e52b503d97400257d6a4df7c6d4e9b6c8c559d9a
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/02/20   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Moniter DIMM throttled after BOM boot complete.
    2. [Feature] Enable BIOS settings on web.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC000502
* GIT repository        : ami_lts_v12_update_3
* GIT version           : f2dffe76691b46badc52f04d4b3f7aaa3aa520c3
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/02/14   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Disable BIOS settings on web for post code hang A7 issue.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. This is a beta version.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC000402
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 5c96da30e61fbf1ea83bc4d566599c1230be94eb
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/02/13   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Fixed] Cannot power on after update BIOS firmware by BMC web.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. This is a beta version.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC000302
* GIT repository        : ami_lts_v12_update_3
* GIT version           : f31ffa69b7c23d49ee36d1c404e284f9d523e470
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacken Lee
* Approved By           :
* RELEASE DATE          : 2025/02/10   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Fixed] Monitor DIMM presence after ROM boot complete.
    2. [Fixed] Disable CPU throttled event due to CPU self-tuning.
    3. [Feature] Prevent DIMM presence event asserted after AC cycle.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. This is a beta version.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC000202
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 2460569ec8c9c15e4fac9d38450bcaeeff6ebab2
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/01/24   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Update Product ID to 3061.
    2. [Fixed] Manual set FAN speed and will go up after a while.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. This is a beta version.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : 3060TUC010802
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 4089e33602f94512acf0b1e13aecfb6112a045df
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/01/23   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Update Product ID to 3060.

Note:
    1. The first four byte "3060" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. Due to SDR changed, do not preserve configuration when update BMC firmware.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC010502
* GIT repository        : ami_lts_v12_update_3
* GIT version           : ae379b3ee39db6a7afae4d3395296ed4e5c6e717
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2025/01/23   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Update Product ID to 3061.
    2. [Feature] Redirect HTTP to HTTPS when login web by browser.
    3. [Fixed #8760] The sensor reading of DIMMs are not in order.
    4. [Fixed] DIMM status presence deasserted and asserted in a short time.

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. Due to SDR changed, do not preserve configuration when update BMC firmware.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : 3060TUC010702
* GIT repository        : ami_lts_v12_update_3
* GIT version           : edef9a4228e5acc44cedaaad4504680450b3f467
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2024/11/22   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [3060][Feature] Support NVMe LED control.

Note:
    1. The first four byte "3060" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. Due to SDR changed, do not preserve configuration when update BMC firmware.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU 1,3,4,6.
* Firmware REV          : 3061TUC010402
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 421c61bae29c1be4c62cd576366221e5fc2a57bf
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2024/11/22   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Common][Feature] Support SNMP community string setting page in settings/SNMP Community String with the permission of "admin" privilege only.
    2. [Common][Feature] Support SNMP Version 1,2,3 selection in Settings/Platform Event Filters/LAN Destinations/LAN Destination Configuration.
    3. [Common][Feature] Support SNMP V2c,V3 command and trap.
    4. [Common][Feature] Support RAID management function in Settings/RAID management page.
    5. [Common][Feature] Implement data download on web.
    6. [Common][Feature] Improve web system inventory.
    7. [Common][Feature] Implement watchdog discrete sensor.
    8. [Common][Feature] Implement negative temperature reading.
    9. [Common][Feature] Implement discrete sensors on web dashboard.
    10. [Common][Feature] Implement BIOS Onetime boot setting in web page.
    11. [Common][Feature] Sort PCIe card by vendor name.
    12. [Common][Feature] Support CPU_Event sensor.
    13. [Common][Feature] Support DIMM_Status sensor.
    14. [Common][Feature] Add all EEPROM data in WebUI download data
    15. [Common][Feature] AFE setting implementation.
    16. [Common][Fix] DIMM sensor name is different with PCB name.
    17. [Common][Fix] Fix Redfish update BMC will trigger WDT2 reset.
    18. [Common][Fix] Updated maximum allowed characters for password in first time login page.
    19. [Common][Fix] BIOS showed unknown BMC IP after setting BMC IP in BIOS setup page

Note:
    1. The first four byte "3061" of Firmware REV is the product ID for this firmware only.
    2. Supported MIB Version: v1.0 or v1.0.*.  Please find AIC MIB file in SNMP_MIB_File directory.
    3. Due to SDR changed, do not preserve configuration when update BMC firmware.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : HA401TU010602
* GIT repository        : ami_lts_v12_update_3
* GIT version           : d190fba5f7d8d27b521f79be42d38ed4231b1d6a
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2024/10/14   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. Change firmware revision.

Note:
    1. Please verify with BIOS firmware version Tuch0050 or above.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : HA401TU000102
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 522d570e9fb62f25505c753e614445a3cb4d2fae
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2024/10/04   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Add PPIN (Protected Identification Number) in System Inventory.
    2. [Feature] [WebUI] Enable BIOS settings on web.
    3. [Fix] Change logrotate.conf to limit size to 50KB.
    4. [Fix] Updated maximum allowed characters for password in first time login page.

Note:
    1. This is a beta version.
    2. Please verify with BIOS firmware version Tuch0050 or above.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : HA401TU010502
* GIT repository        : ami_lts_v12_update_3
* GIT version           : b8a273e88765a3ed0986df57b0ee3e587d6b2d39
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2024/02/26   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Set bonding setting to disable by default.
    2. [Fixed #6660] Update smart FAN table.
    3. [Fixed #6662] Update setconfig default to preserveconfig.

Note:

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU SKU2 and SKU5.
* Firmware REV          : HA401TU010402
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 85f241f975cf029d3bbe9e6058ee536e24361407
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Jacky Liu
* Approved By           : Jacken Lee
* RELEASE DATE          : 2023/12/15   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Feature] Power capping will be enabled for SKU1, 2 and 3.
    2. [Feature] PSU_Watt threshold value depends on different SKU version.
    3. [Fixed] FAN speed did not increase while NVMe drive over temperature.

Note:
    1. Due to updating SDR, please do not preserve config while updating firmware.

*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU
* Firmware REV          : HA401TU010302
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 11cf8c049b07b2c846b356cda1e7c505f5c224aa
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Howard Chang
* Approved By           : Jacken Lee
* RELEASE DATE          : 2023/08/04   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Fixed #6007] Doing cycling ,BMC sel timestamp error reading

Note:


*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU
* Firmware REV          : HA401TU010202
* GIT repository        : ami_lts_v12_update_3
* GIT version           : 399b9666a6204ceb9639255a3ca58e744af45777
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Howard Chang
* Approved By           : Jacken Lee
* RELEASE DATE          : 2023/06/09   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. [Fixed #5785] Unplug the psu, the sel log does not show the psu not detected event.
    2. [Feature] Add unified user account for redfish & IPMI.
    3. [Feature] Setupall.sh is included into FW image now.
    4. [Feature] All fan will push max speed when any node is absent.
    5. [Feature] Add PMBus PEC checking support.
Note:


*****************************************************************
*           BMC firmware release note
*****************************************************************
* Platform              : HA401-TU
* Firmware REV          : HA401TU010102
* GIT repository        : ami_lts_v12_update_3
* GIT version           : a8baccb6745d23988a9cb6ac977b9165a1d65243
* BMC CHIP              : AST2500
* Auxiliary REV         : 2
* IPMI VER              : IPMI 2.0
* Engineer              : Howard Chang
* Approved By           : Jacken Lee
* RELEASE DATE          : 2023/03/28   (YYYY/MM/DD)
*****************************************************************
HISTORY:
    1. First release of HA401-TU.
Note:
    1. Please configure BIOS setup menu “Hardware p-states” from native to disable for P-State power capping.
