AIC-PET-MIB DEFINITIONS ::= BEGIN
	IMPORTS
		enterprises
			FROM RFC1155-SMI
		OBJECT-TYPE
			FROM RFC-1212
        TRAP-TYPE
		    FROM RFC-1215;

	wiredformgmt    OBJECT IDENTIFIER ::= { enterprises 3183 }
	pet             OBJECT IDENTIFIER ::= { wiredformgmt 1 }

	specificTrap	OBJECT IDENTIFIER ::= { pet 1 }
	varBind			OBJECT IDENTIFIER ::= { specificTrap 1 }
	
trapUnderTemperatureWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Under-Temperature Warning (Lower non-critical, going low)"
    ::= 65792

trapTemperatureRecoveredLNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Recovered (Lower non-critical, going high)"
    ::= 65793

trapUnderTemperatureCritical TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Critical Under-Temperature Problem (Lower Critical - going low)"
    ::= 65794

trapTemperatureLowWarningCritWarnLCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Temperature Low Warning: (Lower critical going high)."
    ::= 65795

trapTemperatureLowCriticalCritNonRecoverLNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Temperature Low Critical (Lower non-recover going low)."
    ::= 65796

trapTemperatureLowCriticalNonRecoverCritLNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Temperature Low Critical (Lower non-recover going high)."
    ::= 65797

trapTemperatureRecoveredUNCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Recovered (Upper non-critical going low)"
    ::= 65798

trapOverTemperatureWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Over-Temperature Warning (Upper non-critical, going high)"
    ::= 65799

trapTempHighWarningCritWarnUCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Temperatur High Warning: (Upper critical going low)"
    ::= 65800

trapOverTemperatureCritical TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Critical Over-Temperature Problem (Upper Critical - going high)"
    ::= 65801

trapTempHighCriticalNonRecoverCritUNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Temperatur High Critical: (Upper non-recover going low)"
    ::= 65802

trapTempHighCriticalCritNonRecoverUNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Temperatur High Critical: (Upper non-recover going high)"
    ::= 65803

trapUnderTemperatureWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Under-Temperature Warning Cleared"
    ::= 65920

trapTemperatureRecoveredLNCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Recovered (Lower non-critical, going high) Cleared"
    ::= 65921

trapUnderTemperatureCriticalCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Critical Under-Temperature Problem (Lower Critical - going low) Cleared"
    ::= 65922

trapTemperatureLowWarningCritWarnLCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Low Warning: (Lower critical going high) Cleared."
    ::= 65923

trapTemperatureLowCriticalCritNonRecoverLNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Low Critical (Lower non-recover going low) Cleared."
    ::= 65924

trapTemperatureLowCriticalNonRecoverCritLNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Low Critical (Lower non-recover going high) Cleared."
    ::= 65925

trapTemperatureRecoveredUNCGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperature Recovered (Upper non-critical going low)"
    ::= 65926

trapOverTemperatureWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Over-Temperature warning Cleared"
    ::= 65927

trapOverTemperatureCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Over-Temperature Problem Cleared"
    ::= 65929

trapTempHighCriticalNonRecoverCritUNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperatur High Critical: (Upper non-recover going low) Cleared"
    ::= 65930

trapTempHighCriticalCritNonRecoverUNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Temperatur High Critical: (Upper non-recover going high) Cleared"
    ::= 65931

trapGenericCriticalTemperature TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Generic Critical Temperature Problem (Transition to Critical from less severe)"
    ::= 67330

trapGenericTemperatureWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Generic Temperature Warning (Transition to Warning from less severe)"
    ::= 67331

trapUnderVoltageWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Under-Voltage Warning (Lower Non-Critical - going low)"
    ::= 131328

trapVoltageRecoveredLNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Recovered (Lower non-critical, going high)"
    ::= 131329

trapUnderVoltageCritical TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Critical Under-Voltage Problem (Lower Critical - going low)"
    ::= 131330

trapVoltageLowNoLongerCriticalLCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Low - no longer Critical: (Lower critical going high)"
    ::= 131331

trapVoltageLowCriticalCritNonRecoverLNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Voltage Low - Critical (Lower non-recover going low)"
    ::= 131332

trapVoltageLowCriticalNonRecoverCritLNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Voltage Low - Critical (Lower non-recover going high)"
    ::= 131333

trapVoltageRecoveredUNCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Recovered (Upper non critical going low)"
    ::= 131334

trapOverVoltageWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Over-Voltage Warning (Upper Non-Critical - going high)"
    ::= 131335

trapVoltageHighNoLongerCriticalUCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage High - no longer Critical: (Upper critical going low)"
    ::= 131336

trapOverVoltageCritical TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Critical Over-Voltage Problem (Upper Critical - going high)"
    ::= 131337

trapVoltageHighCriticalNonRecoverCritUNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Voltage High - Critical: (Upper non-recover going low)"
    ::= 131338

trapVoltageHighCriticalCritNonRecoverUNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Voltage High - Critical: (Upper non-recover going high)"
    ::= 131339

trapUnderVoltageWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Under-Voltage Warning Cleared"
    ::= 131456

trapVoltageRecoveredLNCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Recovered (Lower non-critical, going high) Cleared"
    ::= 131457

trapUnderVoltageCriticalCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Under-Voltage Problem Cleared"
    ::= 131458

trapVoltageLowNoLongerCriticalLCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Low - no longer Critical: (Lower critical going high) Cleared"
    ::= 131459

trapVoltageLowCriticalCritNonRecoverLNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Low - Critical (Lower non-recover going low) Cleared"
    ::= 131460

trapVoltageLowCriticalNonRecoverCritLNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Low - Critical (Lower non-recover going high) Cleared"
    ::= 131461

trapVoltageRecoveredUNCGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage Recovered (Upper non critical going low) Cleared"
    ::= 131462

trapOverVoltageWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Over-Voltage Warning Cleared"
    ::= 131463

trapVoltageHighNoLongerCriticalUCGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage High - no longer Critical: (Upper critical going low) Cleared"
    ::= 131464

trapOverVoltageCriticalCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Over-Voltage Problem Cleared"
    ::= 131465

trapVoltageHighCriticalNonRecoverCritUNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage High - Critical: (Upper non-recover going low) Cleared"
    ::= 131466

trapVoltageHighCriticalCritNonRecoverUNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Voltage High - Critical: (Upper non-recover going high) Cleared"
    ::= 131467

trapGenericCriticalDiscreteVoltageCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Generic Critical Voltage Problem Cleared"
    ::= 131840

trapGenericCriticalDiscreteVoltage TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Generic Critical Voltage Problem (Transition to Critical from less severe)"
    ::= 131841

trapGenericCriticalDiscreteVoltage2 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Generic Critical Voltage Problem (Transition to Critical from less severe)"
    ::= 132866

trapGenericDiscreteVoltageWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Generic Voltage Warning (Transition to Non-Critical from less severe)"
    ::= 132867

trapCurrentLowWarningLNCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Current Low Warning (Lower non critical going low)"
    ::= 196864

trapCurrentRecoveredLNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Current Recovered (Lower non critical going high)"
    ::= 196865

trapCurrentCriticalLowLCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current Critical Low (Lower critical going low)"
    ::= 196866

trapCurrentNoLongerCriticalButLowLCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Current no longer Critical but Low (Lower critical going high)"
    ::= 196867

trapCurrentLowDamageLNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current Low Damage (Lower non-recover going low)"
    ::= 196868

trapCurrentNoLongerDamageButCriticalLowLNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current no longer Damage but Critical Low (Lower non-recover going high)"
    ::= 196869

trapCurrentRecoveredUNCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Current Recovered (Upper non critical going low)"
    ::= 196870

trapCurrentHighWarningUNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Current High Warning (Upper non critical going high)"
    ::= 196871

trapCurrentNoLongerCriticalButHighUCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Current no longer Critical but High (Upper critical going low)"
    ::= 196872

trapCurrentHighCriticalUCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current High Critical (Upper critical going high)"
    ::= 196873

trapCurrentNoLongerDamageButCriticalHighUNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current no longer Damage but Critical High (Upper non-recover going low)"
    ::= 196874

trapCurrentHighDamageUNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Current High Damage (Upper non-recover going high)"
    ::= 196875

trapFanUnderSpeedWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Fan speed warning (Fan speed below expected speed)"
    ::= 262400

trapFanIsWorkingOKLNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Recovered (Lower non critical going high)"
    ::= 262401

trapFanCriticalUnderSpeed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Generic Critical Fan Failure (Transition to Critical from less severe)"
    ::= 262402

trapFanPreFailCritWarnLCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Fan Pre-Fail: (Lower critical going high)"
    ::= 262403

trapFanFailedCritNonRecoverLNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan Failed (Lower non-recover going low)"
    ::= 262404

trapFanFailedNonRecoverCritLNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan Failed (Lower non-recover going high)"
    ::= 262405

trapFanRecoveredUNCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Recovered (Upper non critical going low)"
    ::= 262406

trapFanHighWarningUNCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Fan High Warning (Upper non critical going high)"
    ::= 262407

trapFanNoLongerCriticalButHighUCGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan no longer Critical but High (Upper critical going low)"
    ::= 262408

trapFanHighCriticalUCGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan High Critical (Upper critical going high)"
    ::= 262409

trapFanNoLongerDamageButCriticalHighUNRGL TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan no longer Damage but Critical High (Upper non-recover going low)"
    ::= 262410

trapFanHighDamageUNRGH TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan High Damage (Upper non-recover going high)"
    ::= 262411

trapFanUnderSpeedWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan speed Warning Cleared"
    ::= 262528

trapFanIsWorkingOKLNCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Recovered (Lower non critical going high) Cleared"
    ::= 262529

trapFanCriticalUnderSpeedCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Critical Fan Failure Cleared"
    ::= 262530

trapFanPreFailCritWarnLCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Pre-Fail: (Lower critical going high) Cleared"
    ::= 262531

trapFanFailedCritNonRecoverLNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Failed (Lower non-recover going low) Cleared"
    ::= 262532

trapFanFailedNonRecoverCritLNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Failed (Lower non-recover going high) Cleared"
    ::= 262533

trapFanRecoveredUNCGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan Recovered (Upper non critical going low) Cleared"
    ::= 262534

trapFanHighWarningUNCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan High Warning (Upper non critical going high) Cleared"
    ::= 262535

trapFanNoLongerCriticalButHighUCGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan no longer Critical but High (Upper critical going low) Cleared"
    ::= 262536

trapFanHighCriticalUCGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan High Critical (Upper critical going high) Cleared"
    ::= 262537

trapFanNoLongerDamageButCriticalHighUNRGLCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan no longer Damage but Critical High (Upper non-recover going low) Cleared"
    ::= 262538

trapFanHighDamageUNRGHCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan High Damage (Upper non-recover going high) Cleared"
    ::= 262539

trapFanFullRedundancy TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Fan redundancy has returned to Normal"
    ::= 264960

trapFanRedundancyLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fan Redundancy has been Lost"
    ::= 264961

trapFanRedundancyDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Fan Redundancy is in a degraded state"
    ::= 264962

trapPowerSupplyFullRedundancy TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply Redundancy Has Returned to Normal"
    ::= 527104

trapPowerSupplyRedundancyLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Supply Redundancy has been Lost"
    ::= 527105

trapPowerSupplyRedundancyDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Supply Redundancy is in a degraded state"
    ::= 527106

trapPowerUnitRedundancyOk TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Unit Redundancy has been restored"
    ::= 592640

trapPowerUnitRedundancyLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Unit Redundancy has been Lost"
    ::= 592641

trapOEMTransitionToIdle TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to idle"
    ::= 12583424

trapOEMTransitionToActive TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to active"
    ::= 12583425

trapOEMTransitionToBusy TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to busy"
    ::= 12583426

trapOEMStateDeasserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] state deasserted"
    ::= 12583680

trapOEMStateAsserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] state asserted"
    ::= 12583681

trapOEMPredictiveFailureDeasserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] predictive failure deasserted"
    ::= 12583936

trapOEMPredictiveFailureAsserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] predictive failure asserted"
    ::= 12583937

trapOEMLimitNotExceeded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] limit not exceeded"
    ::= 12584192

trapOEMLimitExceeded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] limit exceeded"
    ::= 12584193

trapOEMPerformanceMet TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] performance met"
    ::= 12584448

trapOEMPerformanceLags TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] performance lags"
    ::= 12584449

trapOEMTransitionToOk TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to ok"
    ::= 12584704

trapOEMTransitionToNonCriticalFromOk TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] transition to non critical from ok"
    ::= 12584705

trapOEMTransitionToCriticalFromLessSevere TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] transition to critical from less severe"
    ::= 12584706

trapOEMTransitionToNonRecoverableFromLessSevere TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] transition to non recoverable from less severe"
    ::= 12584707

trapOEMTransitionToNonCriticalFromMoreSevere TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] transition to non critical from more severe"
    ::= 12584708

trapOEMTransitionToCriticalFromNonRecoverable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] transition to critical from non recoverable"
    ::= 12584709

trapOEMTransitionToNonRecoverable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] transition to non recoverable"
    ::= 12584710

trapOEMMonitor TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] monitor"
    ::= 12584711

trapOEMInformational TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] informational"
    ::= 12584712

trapOEMDeviceRemovedDeviceAbsent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] device removed device absent"
    ::= 12584960

trapOEMDeviceInsertedDdevicePresent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] device inserted device present"
    ::= 12584961

trapOEMDeviceDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] device disabled"
    ::= 12585216

trapOEMDeviceEnabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] device enabled"
    ::= 12585217

trapOEMTransitionTorRunning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to rRunning"
    ::= 12585472

trapOEMTransitionToInTest TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to in test"
    ::= 12585473

trapOEMTransitionToPowerOff TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to power off"
    ::= 12585474

trapOEMTransitionToOnLine TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to on line"
    ::= 12585475

trapOEMTransitionToOffLine TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to off line"
    ::= 12585476

trapOEMTransitionToOffDuty TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to off duty"
    ::= 12585477

trapOEMTransitionToDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] transition to degraded"
    ::= 12585478

trapOEMTransitionToPowerSave TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] transition to power save"
    ::= 12585479

trapOEMInstallError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] install error"
    ::= 12585480

trapOEMFullyRedundantRedundancyRegained TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] fully redundant redundancy regained"
    ::= 12585728

trapOEMRedundancyLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] redundancy lost"
    ::= 12585729

trapOEMRedundancyDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] redundancy degraded"
    ::= 12585730

trapOEMNonRedundantSufficientResourcesFromRedundant TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] non redundant sufficient resources from redundant"
    ::= 12585731

trapOEMNonRedundantSufficientResourcesFromInsufficientResources TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] non redundant sufficient resources from insufficient resources"
    ::= 12585732

trapOEMNonRedundantInsufficientResources TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] non redundant insufficient resources"
    ::= 12585733

trapOEMRedundancyDegradedFromFullyRedundant TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] redundancy degraded from fully redundant"
    ::= 12585734

trapOEMRedundancyDegradedFromNonRedundant TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] redundancy degraded from non redundant"
    ::= 12585735

trapOEMD0PowerState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] d0 power state"
    ::= 12585984

trapOEMD1PowerState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] d1 power state"
    ::= 12585985

trapOEMD2PowerState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] d2 power state"
    ::= 12585986

trapOEMD3PowerState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] d3 power state"
    ::= 12585987

trapChassisIntrusion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Chassis Open"
    ::= 356096

trapDriveBayIntrusion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Drive Bay Open"
    ::= 356097

trapIOAreaIntrusion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] I/O Card Area Open"
    ::= 356098

trapProcessorAreaIntrusion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Processor Area Open"
    ::= 356099

trapLANDisconnect TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] LAN Disconnected"
    ::= 356100

trapUnautorizedDock TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Docking Permission Deasserted"
    ::= 356101

trapFANAreaIntrusion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] FAN Area Open"
    ::= 356102

trapChassisIntrusionClosed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Chassis Closed"
    ::= 356224

trapSecureModeViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Secure Mode Violation"
    ::= 421632

trapPrebootUserPasswordViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Pre-boot User password violation"
    ::= 421633

trapPrebootSetupPasswordViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Pre-boot Setup password violation"
    ::= 421634

trapNetworkBootPasswordViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Network Boot Password Violation"
    ::= 421635

trapPasswordViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Password Violation"
    ::= 421636

trapOutOfBandPasswordViolation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Out-of-band Password Violation"
    ::= 421637

trapProcessorInternalError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Processor Internal Error"
    ::= 487168

trapProcessorThermalTrip TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Over Temperature Condition Detected for Processor)"
    ::= 487169

trapProcessorBistError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Processor Failed - FRB1/BIST"
    ::= 487170

trapProcessorFRB2Failure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Processor Failed - FRB2/POST"
    ::= 487171

trapProcessorFRB3Failure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Processor Failed - FRB3"
    ::= 487172

trapProcessorConfigError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Processor Configuration Mismatch"
    ::= 487173

trapSMBIOSUncorrectableCPUComplexError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] SMBIOS Uncorrectable CPU Complex Error asserted"
    ::= 487174

trapProcessorAdded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Added"
    ::= 487175

trapCPUDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] CPU Disabled"
    ::= 487176

trapProcessorTerminatorDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Terminator Detected"
    ::= 487177

trapProcessorThrottle TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Processor Degraded"
    ::= 487178

trapMachineCheckExceptionUncorrectable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Machine Check Exception"
    ::= 487179

trapCorrectableMachineCheckError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Correctable Machine Check Error"
    ::= 487180

trapProcessorInternalErrorCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Internal Error Cleared"
    ::= 487296

trapProcessorThermalTripCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Over Temperature Condition Removed for Processor"
    ::= 487297

trapProcessorBistErrorCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Recovered from FRB1/BIST"
    ::= 487298

trapProcessorConfigErrorCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Recovered - Configuration Mismatch"
    ::= 487301

trapProcessorThrottleCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Processor Not Degraded"
    ::= 487306

trapPowerSupplyPresenceDeteced TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply Inserted"
    ::= 552704

trapPowerSupplyFailureDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power supply Failure detected"
    ::= 552705

trapPowerSupplyWarning TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power supply Warning"
    ::= 552706

trapPowerSupplyACLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Supply AC Lost"
    ::= 552707

trapPowerSupplyInputLostOrOutOfRange TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Supply input lost or out of range"
    ::= 552708

trapPowerSupplyInputOutOfRange TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Supply input out of range"
    ::= 552709

trapPowerSupplyConfigurationError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Supply Configuration Error"
    ::= 552710

trapPowerSupplyPresenceRemoved TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Supply Removed"
    ::= 552832

trapPowerSupplyFailureCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply Failure Cleared"
    ::= 552833

trapPowerSupplyWarningCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply Warning Cleared"
    ::= 552834

trapPowerSupplyACBack TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= 552835

trapPowerSupplyInputOKOrWithinRange TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= 552836

trapPowerSupplyInputOKfromOutofrange TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply input normal"
    ::= 552837

trapPowerSupplyConfigOK TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Supply configuration is OK"
    ::= 552838

trapPowerUnitPowerOffPowerDown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Unit Disabled"
    ::= 618240

trapPowerUnitPowerCycleAsserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Unit power cycled"
    ::= 618241

trapPowerUnit240VAPowerDown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Unit 240VA power down error"
    ::= 618242

trapInterlockPowerDown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Unit Interlock power down error"
    ::= 618243

trapPowerUnitACLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Power Unit power lost"
    ::= 618244

trapPowerUnitSoftPowerControlFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Unit soft power control failed"
    ::= 618245

trapPowerUnitFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Unit failed"
    ::= 618246

trapPowerUnitPredictiveFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Power Unit Predictive Failure"
    ::= 618247

trapMemoryCorrectableECC TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Memory Corrected Error Detected"
    ::= 814848

trapMemoryUncorrectableECC TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Memory uncorrectable error detected"
    ::= 814849

trapMemoryParityError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Memory Parity Error Detected"
    ::= 814850

trapMemoryScrubFailed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Memory Scrub Failure"
    ::= 814851

trapMemoryDeviceDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Memory Disabled"
    ::= 814852

trapMemoryECCLoggingLimitReached TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Memory Logging Limit Reached"
    ::= 814853

trapMemoryPresenceDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Memory Added"
    ::= 814854

trapMemoryConfigurationError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Memory DIMM Configuration Error"
    ::= 814855

trapMemorySpare TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Memory double chip sparing initiated"
    ::= 814856

trapMemoryThrottled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Memory Throttled"
    ::= 814857

trapMemoryCriticalOvertemperature TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Over Temperature Condition Detected for Memory"
    ::= 814858

trapDriveDriveAdded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Drive Added"
    ::= 880384

trapDriveDriveFault TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Drive Disabled due to fault"
    ::= 880385

trapDrivePredictiveFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Array Failure Predicted"
    ::= 880386

trapDriveHotSpare TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Hot Spare Enabled"
    ::= 880387

trapDriveConsistencyCheckInProgress TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Consistency Check Begun"
    ::= 880388

trapDriveInCriticalArray TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Array Critical"
    ::= 880389

trapDriveInFailedArray TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Failed Array"
    ::= 880390

trapDriveRebuildRemapInProgress TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Rebuild in Progress"
    ::= 880391

trapDriveRebuildRemapAbortedwasNotCompletedNormally TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Rebuild Aborted"
    ::= 880392

trapPostError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Post Error"
    ::= 1011456

trapSystemFirmwareHang TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] System Firmware Hang"
    ::= 1011457

trapSystemFirmwareProgress TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System Firmware Progress"
    ::= 1011458

trapCorrectableMemoryErrorLoggingDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Memory Logging Disabled"
    ::= 1076992

trapEventLoggingDisablede TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Event Logging Disabled"
    ::= 1076993

trapLogCleared TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Log Cleared"
    ::= 1076994

trapAllEventLoggingDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] All Event Logging Disabled"
    ::= 1076995

trapLogFull TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Log Full"
    ::= 1076996

trapLogAlmostFull TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Log Almost Full"
    ::= 1076997

trapCorrectableMachineCheckErrorLoggingDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Correctable Machine Check Error Logging Disabled"
    ::= 1076998

trapBIOSWatchdogReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] BIOS Watchdog Reset"
    ::= 1142528

trapOSWatchdogReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog Reset"
    ::= 1142529

trapOSWatchdogShutdown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog Shutdown"
    ::= 1142530

trapOSWatchdogPowerDown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog Power Down"
    ::= 1142531

trapOSWatchdogPowerCycle TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog Power Cycle"
    ::= 1142532

trapOSWatchdogNMIDiagnosticInterrupt TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog NMI / Diagnostic Interrupt"
    ::= 1142533

trapOSWatchdogExpired TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] OS Watchdog Expired, status only"
    ::= 1142534

trapOSWatchdogPretimeoutInterruptNonNMI TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] OS Watchdog pre-timeout Interrupt, non-NMI"
    ::= 1142535

trapSystemReconfigured TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] System Reconfigured"
    ::= 1208064

trapOEMSystemBootEvent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] OEM System Boot Event"
    ::= 1208065

trapUnknownSystemHardwareFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Unknown System Hardware Failure"
    ::= 1208066

trapAuxiliaryLogEntryEvent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Auxiliary Log Entry Event"
    ::= 1208067

trapPEFActionExecuted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] PEF Action Executed"
    ::= 1208068

trapTimestampClockSynch TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Timestamp Clock Synch"
    ::= 1208069

trapFrontPanelNMIDiagnosticInterrupt TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Front Panel NMI / Diagnostic Interrupt"
    ::= 1273600

trapBusTimeout TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Bus Timeout"
    ::= 1273601

trapIOChannelNMI TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] IO Channel check NMI"
    ::= 1273602

trapSoftwareNMI TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] software NMI"
    ::= 1273603

trapPCIPERR TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] PCI PERR"
    ::= 1273604

trapPCISERR TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] PCI SERR"
    ::= 1273605

trapBusUncorrectError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Bus Uncorrectable Error"
    ::= 1273608

trapFatalNMI TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Fatal NMI"
    ::= 1273609

trapBusFatalError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Bus Fatal Error"
    ::= 1273610

trapBusDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Bus Degraded"
    ::= 1273611

trapPowerButtonPressed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Power Button pressed"
    ::= 1339136

trapSleepButtonPressed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Sleep Button pressed"
    ::= 1339137

trapResetButtonPressed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Reset Button pressed"
    ::= 1339138

trapFRULatchOpen TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU latch open"
    ::= 1339139

trapFRUServiceRequestButton TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU service request button"
    ::= 1339140

trapChassisPowerOnAsserted TRAP-TYPE
	ENTERPRISE specificTrap
	DESCRIPTION
	"[Informational] Chassis Transition to Running - Asserted"

	 ::= 1575424

	trapChassisPowerOffAsserted TRAP-TYPE
	ENTERPRISE specificTrap
	DESCRIPTION
	"[Informational] Chassis Transition to Power Off - Asserted"

	 ::= 1575426

trapSoftPowerControlFailed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Soft Power Control Failed"
    ::= 1666816

trapThermalTrip TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Thermal trip"
    ::= 1666817

trapCableInterconnectIsConnected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Cable Interconnect is connected"
    ::= 1798016

trapConfigurationError TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Configuration Error - Incorrect cable connected / Incorrect interconnection"
    ::= 1798017

trapSystemInitiatedByPowerUp TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System Initiated by PowerUp"
    ::= 1928960

trapSystemInitiatedByHardReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System Initiated by Hard Reset"
    ::= 1928961

trapSystemInitiatedByWarmReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System Initiated by Warm Reset"
    ::= 1928962

trapUserRequestedPXEBoot TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] User requested PXE boot"
    ::= 1928963

trapAutomaticBootToDiagnostic TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Automatic boot to diagnostic"
    ::= 1928964

trapOSRuntimeSoftwareInitiatedHardReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] OS / runtime software initiated hard Reset"
    ::= 1928965

trapOSRuntimeSoftwareInitiatedWarmReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] OS / runtime software initiated warm Reset"
    ::= 1928966

trapSystemRestart TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System Restart"
    ::= 1928967

trapNoBootableMedia TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] No bootable media"
    ::= 1994496

trapNonBootableDisketteLeftInDrive TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Non bootable diskette left in drive"
    ::= 1994497

trapPXEServerNotFound TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] PXE Server not found"
    ::= 1994498

trapInvalidBootSector TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Invalid boot sector"
    ::= 1994499

trapTimeoutWaitingForUserSelectionOfBootSource TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Timeout waiting for user selection of boot source"
    ::= 1994500

trapABootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] A: Boot completed"
    ::= 2060032

trapCBootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] C: Boot completed"
    ::= 2060033

trapPXEBootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] PXE Boot completed"
    ::= 2060034

trapDiagnosticBootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Diagnostic Boot completed"
    ::= 2060035

trapCDROMBootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] CD-ROM Boot completed"
    ::= 2060036

trapROMBootCompleted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] ROM Boot completed"
    ::= 2060037

trapBootCompletedBootDeviceNotSpecified TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Boot completed - boot device not specified"
    ::= 2060038

trapStopDuringOSLoadInitialization TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Stop during OS load / initialization"
    ::= 2125568

trapRuntimeStop TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Run-time Stop"
    ::= 2125569

trapOSGracefulCriticalStop TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] OS Graceful Critical Stop"
    ::= 2125570

trapOSGracefulShutdown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] OS Graceful Shutdown"
    ::= 2125571

trapSoftShutdownInitiatedByPEF TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Soft Shutdown initiated by PEF"
    ::= 2125572

trapAgentNotResponding TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Agent Not Responding"
    ::= 2125573

trapSlotFaultAsserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Fault Status asserted"
    ::= 2191104

trapSlotIdentifyAsserted TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Identify Status asserted"
    ::= 2191105

trapSlotDeviceInstalled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot / Connector Device installed/attached"
    ::= 2191106

trapSlotReadyForDeviceInstallation TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot / Connector Ready for Device Installation"
    ::= 2191107

trapSlotReadyForDeviceRemoval TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot/Connector Ready for Device Removal"
    ::= 2191108

trapSlotPoweredOff TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot Power is Off"
    ::= 2191109

trapSlotRemovalRequest TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot / Connector Device Removal Request"
    ::= 2191110

trapSlotInterlockAssertedlatchNotClosed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Interlock asserted"
    ::= 2191111

trapSlotDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot is Disabled"
    ::= 2191112

trapSlotHoldsSpareDevice TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Slot holds spare device"
    ::= 2191113

trapSystemACPIPowerStateWorkingS0G0 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S0 / G0 working"
    ::= 2256640

trapSystemACPIPowerStateSleepingS1 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S1 sleeping"
    ::= 2256641

trapSystemACPIPowerStateSleepingS2 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S2 sleeping, processor context lost"
    ::= 2256642

trapSystemACPIPowerStateSleepingS3 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S3 sleeping, processor & h/w context lost, memory retained"
    ::= 2256643

trapSystemACPIPowerStateSleepingS4SuspendToDisk TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S4 non-volatile sleep / suspend-to disk"
    ::= 2256644

trapSystemACPIPowerStateSleepingS5SoftOff TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S5 / G2 soft-off"
    ::= 2256645

trapSystemACPIPowerStateSleepingS4S5 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S4 / S5 soft-off, particular S4 / S5 state cannot be determined"
    ::= 2256646

trapSystemACPIPowerStateSleepingG7MechanicalOff TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] G3 / Mechanical Off"
    ::= 2256647

trapSystemACPIPowerStateSleepingS1S2S3 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Sleeping in an S1, S2, or S3 states"
    ::= 2256648

trapSystemACPIPowerStateSleepingG1 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] G1 sleeping"
    ::= 2256649

trapSystemACPIPowerStateSleepingS5ByOverrride TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] S5 entered by override"
    ::= 2256650

trapSystemACPIPowerStateLegacyONState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Legacy ON State"
    ::= 2256651

trapSystemACPIPowerStateLegacyOFFState TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Legacy OFF State"
    ::= 2256652

trapSystemACPIPowerStateInvalid TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System ACPI Power State Invalid"
    ::= 2256653

trapSystemACPIPowerStateUnknown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] System ACPI Power State Unknown"
    ::= 2256654

trapWatchdogTimerExpired TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Timer expired, status only"
    ::= 2322176

trapWatchdogHardReset TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Hard Reset"
    ::= 2322177

trapWatchdogPowerDown TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Power Down"
    ::= 2322178

trapWatchdogPowerCycle TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Power Cycle"
    ::= 2322179

trapWatchdogHardwareWatchdogExpired TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Hardware Watchdog expired"
    ::= 2322180

trapWatchdogTimerInterrupt TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Watchdog Timer Interrupt"
    ::= 2322184

trapPlatformAlertGeneratedPage TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] platform generated page"
    ::= 2322176

trapPlatformAlertGeneratedLANAlert TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] platform generated LAN alert"
    ::= 2387713

trapPlatformAlertEventTrapGenerated TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Platform Event Trap generated, formatted per IPMI PET specification"
    ::= 2387714

trapPlatformAlertGeneratedSNMPTrap TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] platform generated SNMP trap, OEM format"
    ::= 2387715

trapEntityPresent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Entity Present"
    ::= 2453248

trapEntityAbsent TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Entity Absent"
    ::= 2453249

trapEntityDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Entity Disabled"
    ::= 2453250

trapLANHeartbeatLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] LAN Heartbeat Lost"
    ::= 2584320

trapLANHeartbeat TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] LAN Heartbeat"
    ::= 2584321

trapSensorAccessDegraded TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] sensor access degraded or unavailable"
    ::= 2649856

trapControllerAccessDegradedOrUnavailable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Controller access degraded or unavailable"
    ::= 2649857

trapManagementControllerOffline TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Management Controller off-line"
    ::= 2649858

trapManagementControllerUnavailable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Critical] Management Controller unavailable"
    ::= 2649859

trapSensorFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Sensor Failure"
    ::= 2649860

trapFRUFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] FRU Failure"
    ::= 2649861

trapBatteryLowpredictiveFailure TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Battery low (predictive failure)"
    ::= 2715392

trapBatteryFailed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Battery failed"
    ::= 2715393

trapBatteryPresenceDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Battery presence detected"
    ::= 2715394

trapSessionActivated TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Session Activated"
    ::= 2780928

trapSessionDeactivated TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Session Deactivated"
    ::= 2780929

trapInvalidUsernameOrPassword TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Invalid Username or Password"
    ::= 2780930

trapInvalidPasswordDisable TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Invalid password disable"
    ::= 2780931

trapHWChangeDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Hardware change detected with associated Entity"
    ::= 2846464

trapFWOrSWChangeDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Firmware or software change detected with associated Entity"
    ::= 2846465

trapHWIncompatibilityDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Hardware incompatibility detected with associated Entity"
    ::= 2846466

trapFWOrSWIncompatibilityDetected TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Firmware or software incompatibility detected with associated Entity"
    ::= 2846467

trapInvalidUnsupportedHWVersion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Entity is of an invalid or unsupported hardware version"
    ::= 2846468

trapInvalidUnsupportedFWOrSWVersion TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Entity contains an invalid or unsupported firmware or software version"
    ::= 2846469

trapHWChangeSuccessful TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Hardware Change detected with associated Entity was successful"
    ::= 2846470

trapSWOrFWChangeSuccessful TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] Software or F/W Change detected with associated Entity was successful"
    ::= 2846471

trapFRUNotInstalled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] FRU Not Installed"
    ::= 2912000

trapFRUInactive TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] FRU Inactive"
    ::= 2912001

trapFRUActivationRequested TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU Activation Requested"
    ::= 2912002

trapFRUActivationInProgress TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU Activation In Progress"
    ::= 2912003

trapFRUActive TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU active"
    ::= 2912004

trapFRUDeactivationRequested TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU Deactivation Requested"
    ::= 2912005

trapFRUDeactivationInProgress TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Informational] FRU Deactivation In Progress"
    ::= 2912006

trapFRUConnectionLost TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] FRU Communication Lost"
    ::= 2912007

trapOEMSpecific TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] OEM Specific"
    ::= 12611328

trapTransitionToM0 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M0"
    ::= 15757056

trapTransitionToM1 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M1"
    ::= 15757057

trapTransitionToM2 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M2"
    ::= 15757058

trapTransitionToM3 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M3"
    ::= 15757059

trapTransitionToM4 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M4"
    ::= 15757060

trapTransitionToM5 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M5"
    ::= 15757061

trapTransitionToM6 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M6"
    ::= 15757062

trapTransitionToM7 TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Transition to M7"
    ::= 15757063

trapIPMBAdisabledIPMBBDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] IPMB A disabled IPMB B disabled"
    ::= 15822592

trapIPMBAenabledIPMBBDisabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] IPMB A enabled IPMB B disabled"
    ::= 15822593

trapIPMBAdisabledIPMBBEnabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] IPMB A disabled IPMB B enabled"
    ::= 15822594

trapIPMBAenabledIPMBBEnabled TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] IPMB A enabled IPMB B enabled"
    ::= 15822595

trapModuleHandleClosed TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Module handle closed"
    ::= 15888128

trapModuleHandleOpened TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Module handle opened"
    ::= 15888129

trapQuiesced TRAP-TYPE
    ENTERPRISE specificTrap
    DESCRIPTION "[Warning] Quiesced"
    ::= 15888130


END
